ESS-BoB Board Design ToDo

# Schematics

* + 24V power input
* + Brake relay
* + Limit switches circuit
  + + Jumpers (solder or physical) to switch between positive and negative limits
  + + Connect to ESS
* + Step, Dir, Enable to ESS.
* + General purpose I/O from ESS to modular screw terminals.
* + Aux relay outputs (24V)
* + Earth to GND connection: decide what’s best and implement (consult with Zvika)
* + Decoupling for TPL7407L (needed?)
* + Decoupling for 5V of the board
* + 5V and 24V power-on LEDs
* See where additional LEDs could be helpful
* Go over spec document and see if everything is covered
* Add footprints wherever missing

# Schematics DR

* Aux 24V outputs need 24V in the connectors, not ground.
* Aux 24V outputs need a smaller connector (e.g. 3.5mm screw terminal quick connects).
* Nice to have: near each test point from the ESS, add test point of ground.
* Add resistors for step and direction inputs (220 Ω 0805).
* Layout: make cutout in the size of the Ethernet connector
  + Ethernet bottom-left: (2776, 1352)
  + Ethernet top-left (2776, 1991)
* + Error in brake connector: need GND in common and 24V at the NC and NO pins.